**DSL modem**

Nom de utilisateur s2m/339451310-adsl

Mot de passe mamadou

**PPPoE / PPPoA Client Mode**

PPPoE/PPPoA Client Enable Disable

VPI 0

VCI 35

Encapsulating Type LLC/SNAP VC MUX

Protocol PPPoA PPPoE

Modulation Multimode T1.413 G.LITE G.GMT ADSL2(G.992.3) ADSL2 annex M ADSL2+(G.992.5) ADSL2+ annex M

**PPPoE Pass-through**

For Wired LAN Enable Disable

**MAC Address Setting** Default MAC address Specify a MAC Address 7C·39·53:A2·FB·E0

**MPoA (RFC1483/2684) Mode**

**MPoA (RFC1483/2684)** Enable Disable

**DSL Modem Settings**

Encapsulation 1483 Bridged IP LLC 1483 Routed IP LLC 1483 Bridged IP VC-Mux 1483 Routed IP VC-Mux (IPoA)

1483 Bridged IP (IPoE)

VPI 0

VCI 101

Modulation Multimode T1.413 G.LITE G.GMT

ADSL2(G.992.3) ADSL2 annex M ADSL2+(G.992.5) ADSL2+ annex M

**WAN Connection Detection**

Mode ARP Detect Ping Detect Always On

Ping IP

TTL:

Bridge Mode Enable Bridge Mode

**MAC Address Setting** Default MAC Address Specify a MAC Address 7C·39·53:A2·FB·E0

**LAN General Setup**

**Ethernet TCP / IP and DHCP Setup**

**LAN IP Network Configuration**

For NAT Usage

IP Address 192.168.2.1

Subnet Mask 255.255.255.0

**DHCP Server Configuration**

Enable Server Disable Server

Start IP Address 192.168.2.10

IP Pool Counts 2

Gateway IP Address 192.168.2.1

**DNS Server IP Address**

Primary IP Address

Secondary IP Address